**Smart Pos**

**AP03**

**Specification**



**1.Introduction**

AP03 Smart POS machine, android 5.1 operating system,5.0 inch screen touch, super long standby battery capacity is 3200 mah, thermal paper printing, 5 million pixels camera, China telecom 2 g / 3 g/wifi, bluetooth communication, magnetic stripe , induction IC card, contact IC card. Now,this fine workmanship and top quality machine is the best choice in the market.

**2.Features**

* Android 5.1 operating system: adopt the open android system, can let the user a simple and efficient development of the upper application,
* serviceable range : apply chain supermarkets, restaurants, convenience stores, clothing store, premises, bakery, cashier, pay, enters sells saves the business management function.

**3.Technical Specification**

|  |  |
| --- | --- |
| Operating system | android 5.1 |
| RAM | RAM:1GB , FLASH: 8GB |
| Extended stored | Micro SD card interface |
| Display screen | 5.0 inch screen touch |
| Touch screen | Capacitive touch screen, support the electronic signature |
| Printer | Built-in high speed thermal printer |
| Magnetic card reader | Support 1/2/3 tracks, two-way scratch card |
| IC card read-write | 1 Pcs |
| SAM gets stuck | 2 Pcs |
| SIM gets stuck | 1 Pcs |
| Non-contact card reader | Support ISO/IEC 14443 Type A&B, Mifare, felica card, in line with the EMV/PBOC PAYPASS specification |
| USB interface | A Micro USB OTG, compatible with USB2.0 HS standards, a Mini USB serial port |
| Communication | 3 g and 2 g network  Wi-fi communications, support hot spots  Bluetooth communication |
| GPS | Built-in GPS |
| Camera | 5 mega-pixel camera |
| Bar-code reader | Support 1 d / 2 d scanning |
| Multimedia | Support for recording, voice broadcast  Support video playback/recording |
| Password keyboard | Built-in password keyboard (virtual)  Support DES, 3 DES, RSA, SHA - 256 and AES algorithm |
| Battery | Lithium battery: 3600 mah, 3.7 V |
| power adapter | Input: 110 v to 240 v AC / 50 ~ 60 hz  Output: 5 v DC / 2 A  General Micro USB interface |
| Size | 191mm×80mm×46mm |
| Optional accessories | Write a stylus  Base, optional standard base (charging function only) |