**Smart Pos**

**AP03**

**Specification**

 

**1.Introduction**

AP03 Smart POS machine, android 5.1 operating system,5.0 inch screen touch, super long standby battery capacity is 3200 mah, thermal paper printing, 5 million pixels camera, China telecom 2 g / 3 g/wifi, bluetooth communication, magnetic stripe , induction IC card, contact IC card. Now,this fine workmanship and top quality machine is the best choice in the market.

**2.Features**

* Android 5.1 operating system: adopt the open android system, can let the user a simple and efficient development of the upper application,
* serviceable range : apply chain supermarkets, restaurants, convenience stores, clothing store, premises, bakery, cashier, pay, enters sells saves the business management function.

**3.Technical Specification**

|  |  |
| --- | --- |
| Operating system | android 5.1  |
| RAM | RAM:1GB , FLASH: 8GB |
| Extended stored  | Micro SD card interface |
| Display screen  | 5.0 inch screen touch |
| Touch screen | Capacitive touch screen, support the electronic signature |
| Printer  | Built-in high speed thermal printer  |
| Magnetic card reader  | Support 1/2/3 tracks, two-way scratch card  |
| IC card read-write | 1 Pcs |
| SAM gets stuck | 2 Pcs  |
| SIM gets stuck | 1 Pcs |
| Non-contact card reader | Support ISO/IEC 14443 Type A&B, Mifare, felica card, in line with the EMV/PBOC PAYPASS specification  |
| USB interface  | A Micro USB OTG, compatible with USB2.0 HS standards, a Mini USB serial port  |
| Communication  | 3 g and 2 g network Wi-fi communications, support hot spotsBluetooth communication  |
| GPS | Built-in GPS  |
| Camera  | 5 mega-pixel camera |
| Bar-code reader | Support 1 d / 2 d scanning  |
| Multimedia | Support for recording, voice broadcast Support video playback/recording |
| Password keyboard  | Built-in password keyboard (virtual) Support DES, 3 DES, RSA, SHA - 256 and AES algorithm  |
| Battery  | Lithium battery: 3600 mah, 3.7 V  |
| power adapter  | Input: 110 v to 240 v AC / 50 ~ 60 hz Output: 5 v DC / 2 AGeneral Micro USB interface  |
| Size | 191mm×80mm×46mm |
| Optional accessories | Write a stylus Base, optional standard base (charging function only)  |